Technical Data Sheet

Joint Backer Rod  
Polyethylene Foam Material

Description

Backer Rod is a non-absorbent,  
compressible grey closed cell  
polyethylene (P.E) foam   
backup material.

Sizes Available in Grey

6mm x 2500m  
10mm x 1150m  
13mm x 750m  
15mm x 550m  
20mm x 350m  
25mm x 200m  
30mm x 160m  
40mm x 270m  
50mm x 180m

Product Specification

Box quantity – 1 Roll  
Boxes / Pallet – 12

Storage

Store in original container in cool dry conditions, away from direct sunlight.

Shelf Life

Storage life in 12 months in tightly sealed, undamaged containers.

Health & Safety

Non-Hazardous

Benefits

* Quick and easy to apply.
* Reduces sealant usage.
* Improves sealant performanceby obtaining easily the correct   
  joint dimensions.
* Flexible; won’t bubble or blister.

Recommended for

* Reducing the depth or joints in  
  construction / glazing use.
* Creating a backstop to allow  
  proper sealant tooling.

**For technical advice call   
 - 08450 505 986**

**Or email   
- info@completeconstructionproducts**